These firmware's are intended only for Chroma-Q Studio Force II  12, 48 and 72

IMPORTANT
Before updating, check the bootloader version
(See Menu/Setup/FW Version and then then number next to BL (example, BL v1.06)
If the bootloader version is lower than 1.05 please contact Chroma-Q support before attempting to install the firmware.

To install the firmware, a Chroma-Q Uploader II will be needed.
Follow the upload instructions in the included PDF
Note: there are two firmware's per fixture to be updated, the addressing board and the engine boards, the order into which the update is done is not important.
If many fixtures must be updated, only one fixture can be done at once, no serial update, it will corrupt the firmware. 

After the firmware’s are installed, do the following to ensure all settings are nominal.
In the DMX Address menu, enter 555 and press Enter, this will sync the engines with the addressing board
In the menu Setup/Reset, select Default and press and hold Apply until the fixture resets.

Redo the Settings as desire, modes, Options and DMX address and the fixture is ready to be used.

2.3 Changes since the previous release:
•	Fixed Play captured DMX
•	Store user settings upon pressing the Apply button
•	Fixed Gpio configuration on Engine upload
•	GUI cosmetic changes


2.2 Changes since the previous release:
•	 Fixed DMX Lost not holding, 
•	 Fixed DMX Input Store not working and 
•	 Fixed DMX Lost Off not working for CineQ

2.1 Changes since the previous release:
•	Fixed an issue with version/temperature reporting on Studio Force II 48 model

2.0 Changes since the previous release:
•	Needs Engine firmware 3.0 or higher
•	We have improved the very low intensity color distortion.
•	Smoother fade transition 
•	Improved synchronizations between each fixture engine
•	New direct mode for dynamic DMX effect (Smoothing On/Off option in Mode menu and DMX control channel)
•	New Cine-Q option to allow the Auto white in RGBW (Autowhite option in Mode menu and DMX control channel) AutoWhite is a great feature to use with RGB pixelmapping
•	New Inhibitive mode for the white channel in Cine-Q 8b / Cine-Q 16b RGBW control.
	When Autowhite is enabled, the white channel act like an inhibitive to the amount of white LED added to he RGB mix.
•	New menu interface
•	New manual control mode and presets store function


DMX mapping for consoles 
The actual DMX channel layout remains the same, however the functions within the control channel have changed, there are now a few more important functions.

Console fixture profiles might require an update from the console manufacturer, please contact them for such update.

The attached PDF contains the changes as well as a CCT to DMX table and a RGBW to CCT table

For any additional info, contact us at info@Chroma-q.com
