These firmware's are intended only for Chroma-Q Studio Force II Plus 12, 48 and 72
	
IMPORTANT

To install the firmware, a Chroma-Q Uploader II will be needed.
Follow the upload instructions in the included PDF
Note: there are two firmware's per fixture to be updated, the addressing board and the engine boards, the order into which the update is done is not important.
If many fixtures must be updated, only one fixture can be done at once, no serial update, it will corrupt the firmware. 

After the firmware’s are installed, do the following to ensure all settings are nominal.
In the DMX Address menu, enter 555 and press Enter, this will sync the engines with the addressing board
In the menu Setup/Reset, select Default and press and hold Apply until the fixture resets.

Redo the Settings as desire, modes, Options and DMX address and the fixture is ready to be used.


========================================================================================
LED Engine Firmware version: 4.1.0
	•	File Name: StudioForceII_Plus_Eng_App_v4.1.0.bin
	•	Release Date: 2024-08-06
	•	Compatible Engine PCBs: All
	•	Compatible Units: All Studio Force II Plus
	•	Changes since the previous release:

## [v4.1.0] - 2024-08-06
### Changed 
- CCT HUE Plus Green values adjusted.

## [v4.0.1] - 2024-06-17
### Changed 
- Temperature control updated.

## [v4.0.0] - 2024-04-15
- First release for StudioForceII PLUS.
### Added
- Correction table for SFII PLUS rev A Engine.
- Improved smoothing. 



DMX mapping for consoles 
The actual DMX channel layout remains the same, however the functions within the control channel have changed, there are now a few more important functions.

Console fixture profiles might require an update from the console manufacturer, please contact them for such update.

The attached PDF contains the changes as well as a CCT to DMX table and a RGBW to CCT table

For any additional info, contact us at info@Chroma-q.com
